Agora RTC Objective-C API Reference Refactor

Data Fields
CameraCapturerConfiguration Struct Reference

## Data Fields
char | deviceId [MAX_DEVICE_ID_LENGTH]
VideoFormat | format

## Detailed Description

Camera capturer configuration.

## Constructor & Destructor Documentation

## ◆ CameraCapturerConfiguration()

CameraCapturerConfiguration | ( |  | ) |
| inline

## Field Documentation

## ◆ deviceId

char deviceId[MAX_DEVICE_ID_LENGTH]

Camera direction settings (for Android/iOS only). See: CAMERA_DIRECTION. For windows. The device ID of the playback device. The maximum length is #MAX_DEVICE_ID_LENGTH.

## ◆ format

VideoFormat format

The video format. See VideoFormat.

## ◆ followEncodeDimensionRatio

bool followEncodeDimensionRatio