Agora RTC Objective-C API Reference Refactor

Properties
AgoraLastmileProbeConfig Class Reference

Inherits <NSObject>.

## Properties
BOOL | probeUplink
BOOL | probeDownlink
NSUInteger | expectedUplinkBitrate
NSUInteger | expectedDownlinkBitrate

## Detailed Description

The configurations for the last-mile network probe test.

## Property Documentation

## ◆ probeUplink

- (BOOL) probeUplink
| read write nonatomic assign

Sets whether or not to test the uplink network.

Some users, for example, the audience in a live-broadcast channel, do not need such a test.

- `YES`: Enables the test.
- `NO`: Disables the test.

## ◆ probeDownlink

- (BOOL) probeDownlink
| read write nonatomic assign

Sets whether or not to test the downlink network.

- `YES`: Enables the test.
- `NO`: Disables the test.

## ◆ expectedUplinkBitrate

- (NSUInteger) expectedUplinkBitrate
| read write nonatomic assign

Sets the expected maximum sending bitrate (bps) of the local user.

The value ranges between 100000 and 5000000. Agora recommends setting this value according to the required bitrate of selected video profile.

## ◆ expectedDownlinkBitrate

- (NSUInteger) expectedDownlinkBitrate
| read write nonatomic assign

Sets the expected maximum receiving bitrate (bps) of the local user. The value ranges between 100000 and 5000000.