Agora Java API Reference for Android

Public Attributes | List of all members
agora::rtc::TranscodingUser Struct Reference

`#include <AgoraBase.h>`

## Public Attributes
uid_t | uid
int | x
int | y
int | width
int | height
int | zOrder
double | alpha
int | audioChannel

## Detailed Description

Transcoding configurations of each host.

## Member Data Documentation

## ◆ uid

uid_t agora::rtc::TranscodingUser::uid

The user ID of the host.

## ◆ x

int agora::rtc::TranscodingUser::x

The x coordinate (pixel) of the host's video on the output video frame (taking the upper left corner of the video frame as the origin). The value range is [0, width], where width is the `width` set in `LiveTranscoding`.

## ◆ y

int agora::rtc::TranscodingUser::y

The y coordinate (pixel) of the host's video on the output video frame (taking the upper left corner of the video frame as the origin). The value range is [0, height], where height is the `height` set in `LiveTranscoding`.

## ◆ width

int agora::rtc::TranscodingUser::width

The width (pixel) of the host's video.

## ◆ height

int agora::rtc::TranscodingUser::height

The height (pixel) of the host's video.

## ◆ zOrder

int agora::rtc::TranscodingUser::zOrder

The layer index number of the host's video. The value range is [0, 100].

- 0: (Default) The host's video is the bottom layer.
- 100: The host's video is the top layer.

If the value is beyond this range, the SDK reports the error code `ERR_INVALID_ARGUMENT`.

## ◆ alpha

double agora::rtc::TranscodingUser::alpha

The transparency of the host's video. The value range is [0.0, 1.0].

- 0.0: Completely transparent.
- 1.0: (Default) Opaque.

## ◆ audioChannel

int agora::rtc::TranscodingUser::audioChannel

The audio channel used by the host's audio in the output audio. The default value is 0, and the value range is [0, 5].

- `0`: (Recommended) The defaut setting, which supports dual channels at most and depends on the upstream of the host.
- `1`: The host's audio uses the FL audio channel. If the host's upstream uses multiple audio channels, the Agora server mixes them into mono first.
- `2`: The host's audio uses the FC audio channel. If the host's upstream uses multiple audio channels, the Agora server mixes them into mono first.
- `3`: The host's audio uses the FR audio channel. If the host's upstream uses multiple audio channels, the Agora server mixes them into mono first.
- `4`: The host's audio uses the BL audio channel. If the host's upstream uses multiple audio channels, the Agora server mixes them into mono first.
- `5`: The host's audio uses the BR audio channel. If the host's upstream uses multiple audio channels, the Agora server mixes them into mono first.
- `0xFF` or a value greater than 5: The host's audio is muted, and the Agora server removes the host's audio.

Note
  If the value is not `0`, a special player is required.